Rubber Ducky

* When the Rubber Ducky is connected to the PC it gets recognized as HID keyboard and then proceeds to run a series of inputs to launch a file.

USB Valve

* When the USB valve is used to check if the Rubber Ducky is safe. it displays that the device is showing as a HID device and is sending inputs. Which is the red flag, as it’s a USB storage device and should not be sending inputs.

The Potential Harm of the Rubber Ducky

* A employee, or malicious actor could easily gain access to any computer within a company and plug in the Rubber Ducky. Which would install malware on to their PC, or potentially on the whole company’s network. Allowing them remote access and control over a system to retrieve information and lists. Which could be sold or used to extort the company.

